QUESTION:

Write an assembly language program to swap two 8-bit data using 8085 processor

PROGRAM:

lda 2001

mov b,a

lda 2005

sta 2001

mov a,b

sta 2005

hlt

OUTPUT:



